5x8 dot-matrix liquid crystal display based on AiP31068 LCD controller, with I2C interface.

Property: (default value)

- Rows: (2 Rows)
   Number of rows of characters.

- Columns: (16 Columns)
   Number of characters per row.

- I2C Address: (62)
   Device address.

- I2C Frequency: (100 KHz)
   It is better to be similar to I2C Master frequency, but not critical in most cases.
