Sezioni di filettatura standard

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **Raccordo** | **Ø (mm)** | **L (mm)** |
| **Raccordo tubo**Attacco standard per fascetta stringitubo | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-hose.jpg | 6.3 mm (1/4")8 mm (5/16")10 mm (3/8")13 mm (1/2")18 mm (5/8") | ----- | 18.018.021.021.021.0 |
| **Raccordo Stream-line**Attacco per tubo con tenuta conica su maschio e dado  | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-stream-line.jpg | 5 x 8 mm6.5 x 10 mm8 x 12 mm9.5 x 13.5 mm11 x 16 mm | ----- | 15.017.019.021.025.0 |
| **Raccordo CEJN-lock**Per tubo senza graffatura o fascette  | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-cejn-lock.jpg | 1/4"3/8"1/2" | --- | 19.023.026.0 |
| **Filettatura UNF**Filettatura unificata conforme ISO 68, ANSI B1.1Maschio:es. 9/16"-18 UNFFemmina:es. 7/16"-20 UNFFemmina, SEA O-Ring Boss | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-male.jpghttps://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread**7/16"-20 UNF7/8"-14 UNF**Filettatura femmina**7/16"-20 UNF9/16"-18 UNF3/4"-16 UNF1 1/16"-16 UNF1 5/16"-12 UNF | 11.022.09.812.917.526.833.1 | 13.315.511.512.714.319.019.0 |
| **Filettatura Metrica**Filettatura metrica conforme ISO 68 / ISO 724Maschio:es. M16x1.5Femmina:es. M16x1.5 | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-metric-male.jpghttps://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread**M10x1.25M12x1.5M14x1.5M16x1.5M22x1.5**Filettatura femmina**M16x1.5 | 9.811.8513.8515.8521.8514.5 | 9.013.013.08.8115.79.0 |
| **Raccordo filettato R/Rc**Filettatura conica conforme ISO 7/1 (altre descrizioni comuni sono BSPT, Kr) Maschio:es. R 1/4"Femmina:es. Rp 1/4" (cilidrica) es. Rc 1/4" (conica)  | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-r-male.jpghttps://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-rc-female.jpg | **Male Thread**R 1/8"R 1/4"R 3/8"R 1/2"R 3/4"**Filettatura femmina**Rc 1/8"Rc 1/4"Rc 3/8"Rc 1/2"Rc 3/4" | 10.213.617.221.727.18.311.014.518.023.5 | 7.411.011.015.016.37.411.011.415.016.3 |
| **Raccordo filettato G**Filettatura cilindrica conforme ISO 228/1 (altre descrizioni comuni sono BSP, R) Maschio:es. G 1/4" Femmina (ISO 1179):es. G 1/4" | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-g-male_2.jpghttps://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread**G 1/8"G 1/4"G 3/8"G 1/2"G 3/4"**Filettatura femmina**G 1/8"G 1/4"G 3/8"G 1/2"G 3/4" | 9.613.016.520.826.38.7511.815.2519.024.5 | 8.010.010.012.012.07.411.011.415.016.3 |
| **Raccordo filettato NPT**Filettatura standard americana conforme ANSI/ASME B 1.20.1Maschio e Femmina: es. 1/4" NPT | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-npt-male.jpghttps://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-npt-female.jpg | **Male Thread**1/8" NPT1/4" NPT3/8" NPT1/2" NPT3/4" NPT**Filettatura femmina**1/8" NPT1/4" NPT3/8" NPT1/2" NPT3/4" NPT | 10.514.017.521.827.18.511.014.518.023.0 | 6.710.210.413.613.96.910.010.313.614.1 |